{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Feuille 1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Feuille 1","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"merged":[[2,0,8,0],[11,0,13,0],[23,0,24,0]],"flags":["formulas_cached_only"]}
[null,"Données","Valeurs","Informations"]
[]
["Paramètres du cycliste","Poids du cycliste (kg)",70]
[null,"Poids du vélo (kg)",10]
[null,"Poids à déplacer (kg)",80]
[]
[null,"Coefficient de pénétration dans l’air",0.2,"source"]
[]
[null,"frottements mécaniques internes au vélo relatifs au système de transmission des efforts entre les pédales et la roue arrière (chaîne, dérailleur, moyeux).","négligeables"]
[]
[]
["Paramètres de la route","pente de la route (%)"]
[null,"coefficient de frottement de la chaussée (qui s’exprime en équivalent pente et donc en %)",1.5,"Ce coefficient est compris entre 0,5 et 1,5 pour des chaussées normales.","source"]
[null,"vent","négligé"]
[]
[null,"Puissance = (intensité de la force)*(vitesse) "]
[null,"puissance moyenne"]
[null,"travail fourni par le cycliste (en Kilo-Joules)"]
[null,"travail fourni par le cycliste (en watt-heure)"]
[]
[]
[]
[]
["Paramètre de la machine","Vitesse d'essorage tr/min (rpm)",600,"600 / 800 / 1000 / 1200 tr/min (rpm)"]
[null,"Poids du cylindre (kg) dont linge et eau",21]