Partlist exported from /Users/Miros2424/Desktop/EH 400 MINI SYNTH shareware.sch at 2014-12-06 10:38 AM

Assembly variant:

Part | Value | Device | Package | Description
+9_BATT |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
+9_BATT1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
ADDED | 10k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
ADDED1 | 8.2k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
ADDED_C | 1uF (or try diff. values) | CAP_POLPTH2 | CPOL-RADIAL-10UF-25V | Capacitor Polarized
ADDED_C1 | 1uF (or try diff. values) | CAP_POLPTH2 | CPOL-RADIAL-10UF-25V | Capacitor Polarized
AUDIO_GND |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
AUDIO_GND1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
AUDIO_L |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
AUDIO_L1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
AUDIO_R |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
AUDIO_R1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
BOTTOM_NOTE |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
BOTTOM_NOTE1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
C-ADDED | 1uF (or try diff. values) | CAP_POLPTH2 | CPOL-RADIAL-10UF-25V | Capacitor Polarized
C1 | .056 | CAP_ | AXIAL-5MM | Capacitor
C2 | .056 | CAP_ | AXIAL-5MM | Capacitor
C3 | 10uF | CAP_POLPTH1 | CPOL-RADIAL-100UF-25V | Capacitor Polarized
C4 | .001 | CAP_ | AXIAL-5MM | Capacitor
C5 | 10uF | CAP_POLPTH2 | CPOL-RADIAL-10UF-25V | Capacitor Polarized
C6 | 4u7_tantalum | CAP_POLPTH2 | CPOL-RADIAL-10UF-25V | Capacitor Polarized
C7 | 10uF | CAP_POLPTH2 | CPOL-RADIAL-10UF-25V | Capacitor Polarized
C8 | .1 | CAP_ | AXIAL-5MM | Capacitor
C9 | 680p | CAP_ | AXIAL-5MM | Capacitor
C10 | .01 | CAP_ | AXIAL-5MM | Capacitor
C11 | 1uF | CAP_POLPTH1 | CPOL-RADIAL-100UF-25V | Capacitor Polarized
C12 | .033 | CAP_POLPTH2 | CPOL-RADIAL-10UF-25V | Capacitor Polarized
C13 | 680p | CAP_ | AXIAL-5MM | Capacitor
C14 | 10uF | CAP_POLPTH2 | CPOL-RADIAL-10UF-25V | Capacitor Polarized
C15 | .0233 | CAPPTH1 | CAP-PTH-5MM | Capacitor
C16 | 33uF | CAP_POLPTH2 | CPOL-RADIAL-10UF-25V | Capacitor Polarized
C17 | 100uF | CAP_POLPTH1 | CPOL-RADIAL-100UF-25V | Capacitor Polarized
C18 | .015 | CAP_ | AXIAL-5MM | Capacitor
C19 | 220uF | CAP_POLPTH1 | CPOL-RADIAL-100UF-25V | Capacitor Polarized
C20 | .22 tantalum | CAP_POLPTH1 | CPOL-RADIAL-100UF-25V | Capacitor Polarized
D1 |  | DIODE1N4148 | DIODE-1N4148 | Diode
D2 |  | DIODE1N4148 | DIODE-1N4148 | Diode
D3 |  | DIODE1N4148 | DIODE-1N4148 | Diode
D4 | 6.8V | DIODE-ZENERPTH | DIODE-ZENER | Zener Diode
GND_BATT |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
GND_BATT1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
IC1 | LM339N | LM339N | DIL14 | Low Power Low Offset Voltage Quad Comparators
IC2 | CA3094 | LM3080N | DIL08 | OP AMP
IC3 | CA3094 | LM3080N | DIL08 | OP AMP
IC4 | 4013N | 4013N | DIL14 | Dual D FLIP FLOP, set/reset
IC5 | TBS820M | AD744N | DIL08 | Precision, 500 ns Settling BiFET Op Amp
J1 |  | JACK-3.5-3P | PW-3P-3.5-14X9.5-DIP |
JACK_GND |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
JACK_GND1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
JACK_POS |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
JACK_POS1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
LOGO1 | LOGO-OSHW-FILLX0200-NT | LOGO-OSHW-FILLX0200-NT | OSHW_FILLX200_NOTEXT |
OUTPUT |  | AUDIO-JACK2.5MM | STEREOJACK2.5MM_STEREOJACK2.5MM | 3.5mm Audio Jack
PIEZO_GND |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
PIEZO_GND1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
PIEZO_PLUS |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
PIEZO_PLUS1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
PR1-INTONATION | 5k | TRIM_EU-S75P | S75P | POTENTIOMETER
PR2-FINE_TUNE | 5k | TRIM_EU-S75P | S75P | POTENTIOMETER
Q1 | PN4154 | 2N2907 | TO92-EBC-OVAL | PNP Transistor
Q2 | 2N5088 | 2N2222 | TO92-EBC-OVAL | NPN TRANSISTOR
Q3 | 2N5087 | 2N2907 | TO92-EBC-OVAL | PNP Transistor
Q4 | 2N5088 | 2N2222 | TO92-EBC-OVAL | NPN TRANSISTOR
Q5 | 2N5088 | 2N2222 | TO92-EBC-OVAL | NPN TRANSISTOR
Q6 | 2N5088 | 2N2222 | TO92-EBC-OVAL | NPN TRANSISTOR
Q8 | 2N5088 | 2N2222 | TO92-EBC-OVAL | NPN TRANSISTOR
R-ADDED | 1M | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R1 | 33k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R1-1 | 2k7 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-2 | 3k | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-3 | 3k3 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-4 | 3k3 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-5 | 3k3 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-6 | 3k9 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-7 | 3k9 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-8 | 4k3 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-9 | 4k3 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-10 | 4k7 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-11 | 5k1 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-12 | 5k1 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-13 | 5k6 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-14 | 6k2 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-15 | 6k2 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-16 | 6k8 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-17 | 6k8 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-18 | 7k5 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-19 | 8k2 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-20 | 8k2 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-21 | 8k2 | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-22 | 10k | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-23 | 10k | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R1-24 | 10k | RESISTORAXIAL-0.3 | AXIAL-0.3 | Resistor
R2 | 4k7 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R3 | 10k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R4 | 15k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R5 | 30k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R6 | 150k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R7 | 18k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R8 | 22k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R9 | 220k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R10 | 150k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R11 | 130k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R12 | 4k7 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R13 | 220k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R14 | 27k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R15 | 680k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R16 | 12k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R17 | 2k7 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R18 | 4M7 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R19 | 100k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R20 | 10k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R21 | 3k9 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R22 | 1M5 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R23 | 10k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R24 | 10k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R25 | 1M | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R26 | 330k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R27 | 33 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R28 | 270 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R29 | 27k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R30 | 47k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R31 | 10k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R32 | 5k6 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R33 | 1M | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R34 | 330k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R35 | 33 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R36 | 270 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R37 | 27k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R38 | 47k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R39 | 10k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R40 | 5k6 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R41 | 33k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R42 | 4k7 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R43 | 120 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R44 | 10k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R45 | 1 | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R46 | 10k | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
R70 | 1M | RESISTORPTH-1/4W | AXIAL-0.4 | Resistor
S1 | OCTAVE | SWITCH-DPDTOS | OS | DPDT Version of the COM-00597
S2 | PHASE | SWITCH-DPDTOS | OS | DPDT Version of the COM-00597
S3 | SENS | EG1218S | EG1218 | SLIDING SWITCH
S4 | DOUBLE_FILTER | EG1218S | EG1218 | SLIDING SWITCH
S5 | Q | SWITCH-DPDTOS | OS | DPDT Version of the COM-00597
S6 | POWER | EG1218S | EG1218 | SLIDING SWITCH
SP1 | SPEAKER/AL11P | SPEAKER/AL11P | AL11P | SPEAKER Source: BuerklinAdded PS12 (for part # PS1240 piezo) http://www.ladyada.net/library/pcb/eaglelibrary.html
SP2 | SPEAKER/AL11P | SPEAKER/AL11P | AL11P | SPEAKER Source: BuerklinAdded PS12 (for part # PS1240 piezo) http://www.ladyada.net/library/pcb/eaglelibrary.html
SPEAKER_NEG1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
SPEAKER_POS |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
SPEAKER_POS1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
SPEAKR_NEG |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
STILET |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
STILET1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
TOP_NOTE |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
TOP_NOTE1 |  | PINHD-1X1 | 1X01 | Pin header 1x1 for 0.1" spacing
V1 | 9VBATTERY | 9VBATTERY | AB9V |
V2 | 9VBATTERY | 9VBATTERY | AB9V |
VR1-PITCH_BEND | 10k | R-POTENTIOMETER-3362U | 3362U | Potentiometer
VR2-SUB_OCTAVE | 100k | R-POTENTIOMETER-3362U | 3362U | Potentiometer
VR3-PHASE_RATE | 100k | R-POTENTIOMETER-3362U | 3362U | Potentiometer
VR4-SWEEP_START_FREQ | 10k | R-POTENTIOMETER-3362U | 3362U | Potentiometer
VR5-SWEEP_STOP_FREQ | 100k | R-POTENTIOMETER-3362U | 3362U | Potentiometer
VR6-SWEEP_RATE | 100k | R-POTENTIOMETER-3362U | 3362U | Potentiometer
VR7-VOLUME | 100k | R-POTENTIOMETER-3362U | 3362U | Potentiometer