{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["calcul (2)"],"not_rendered":{"images":1,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"calcul (2)","index":0,"n_rows":30,"n_cols":10,"rows_kept":30,"merged":[[1,0,1,6]],"flags":["formulas_cached_only"]}
[]
["Débit-vitesse dans une cana gravitaire"]
[]
[{"$nulls":8},"Ø nominal","Ø interieur"]
[null,"Diamètre intérieur de la canalisation","D= ",0.288,null,"m",null,null,"D100",0.1]
[{"$nulls":8},"D125",0.114]
[null,"pourcentage de remplissage","P= ",{"v":75,"d":"75.00"},null,"%",null,null,"D160",0.146]
[{"$nulls":3}," ",{"$nulls":4},"D200",0.182]
[null,"Pente de la canalisation","I = ",{"v":1,"d":"1.00"},null,"cm/mètre",null,null,"D250",0.228]
[{"$nulls":3},0.01,null,"mètre/mètre",null,null,"D315",0.288]
[{"$nulls":8},"D400",0.365]
[null,"RESULTAT",{"$nulls":6},"D500",0.459]
[]
[null,"débit calculé","Q= ",{"v":0.08714278426319437,"d":"0.08714"},null,"m3/s"]
[{"$nulls":3},{"v":313.71402334749973,"d":"313.71"},null,"m3/h"]
[{"$nulls":3},{"v":87.14278426319437,"d":"87.14"},null,"l/s",{"v":5228.567055791662,"d":"5228.57"},"L/min"]
[null,null," "]
[null,"vitesse","V=",{"v":1.6627659611907413,"d":"1.66"},null,"m/s"]
[]
[]
[null,null,"a = ",{"v":4.1887902047863905,"d":"4.19"},null,"radians"]
[null,"Angle de la longueur mouillée","a = ",{"v":239.99999999999997,"d":"240"},null,"degrés"]
[null,"Rayon de la canalisation","ra = ",0.144,null,"m"]
[null,"Hauteur d'eau dans la canalisation","H = ",{"v":0.21599999999999997,"d":"0.216"},null,"m"]
[null,"périmètre mouillé","Lm = ",{"v":0.60288,"d":"0.603"},null,"m"]
[null,"Rayon hydraulique","R = ",{"v":0.08692994995631362,"d":"0.087"},null,"m"]
[null,"Longueur de la corde","Co = ",{"v":0.24941531628991834,"d":"0.249"},null,"m"]
[null,"Surface du rayon hydraulique","S = ",{"v":0.05240832822966235,"d":"0.052408"},null,"m²"]
[]
[null,"section du tuyau","St = ",{"v":0.06514406526483794,"d":"0.0651"},null,"m²"]