{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Feuille1","Feuille2","Feuille3"],"not_rendered":{"external_links":1,"defined_names":10},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Feuille1","index":0,"n_rows":28,"n_cols":11,"rows_kept":28,"flags":["formulas_cached_only"]}
{"$rows_empty":15}
[{"$nulls":3},"Formule yn=som(EiSiyi)/som(EiSi)"]
["he",0.049]
["be",0.084,null,"moments statiques"]
["hi",0.045,null,"alu",{"v":901753.8600000015,"d":"901,753.86"}]
["bi",0.08,null,"acier",{"v":4006800,"d":"4,006,800.00"},null,"Méthode en utilisant k"]
["ep",0.002,null,"Total",{"v":4908553.860000001,"d":"4,908,553.86"}]
["Eac",{"v":210000000000,"d":"2.10E+011"},{"$nulls":5},"Ms","Ms pond",null,"Surface pond"]
["Eal",{"v":71330000000,"d":"7.13E+10"},null,"Surfaces",null,null,"alu",1.264200000000002e-05,1.264200000000002e-05,null,0.0005160000000000008]
["k",2.944062806673209,null,"alu",{"v":36806280.00000006,"d":"36,806,280.00"},null,"acier",1.764e-05,5.193326790971541e-05,null,0.0021197252208047103]
["ep2a",0.008,null,"acier",{"v":218399999.99999997,"d":"218,400,000.00"},null,null,1.4400000000000002e-06,4.2394504416094215e-06,null,0.0009421000981354269]
["ep2b",0.005,null,"Total",{"v":255206280.00000003,"d":"255,206,280.00"},null,"Total",null,6.881471835132484e-05,null,0.003577825318940138]
[]
[{"$nulls":3},"yn=Ms/S",0.019233671914343175,{"$nulls":3},0.019233671914343175]

{"sheet":"Feuille2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Feuille3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}